

Agricultural Water Use Package for MODFLOW or GSFLOW

By Richard G. Niswonger

Open–File Report 2017–#

Version X.X, Month 201X [if needed]  
Supersedes USGS Series Report XXXX–XXXX [if needed]

U.S. Department of the Interior

RYAN ZINKE, Secretary

U.S. Geological Survey

William Werkheiser, Acting Director

U.S. Geological Survey, Reston, Virginia: 2017

For more information on the USGS—the Federal source for science about the Earth,  
its natural and living resources, natural hazards, and the environment—visit  
<http://www.usgs.gov>/ or call 1–888–ASK–USGS (1–888–275–8747).

For an overview of USGS information products, including maps, imagery, and publications,  
visit <http://www.usgs.gov/pubprod>/.

Any use of trade, firm, or product names is for descriptive purposes only and does not imply  
endorsement by the U.S. Government.

Suggested citation:  
Niswonger, R.G., 2017, Agricultural Irrigation Package for MODFLOW-NWT, U.S. Geological Survey Open File Report 2017-xxx, 13 p,   
<http://dx.doi.org/x>.

ISSN XXXX-XXXX (print) [if applicable]  
ISSN XXXX-XXXX (CD/DVD) [if applicable]  
ISSN XXXX-XXXX (online)  
ISBN XXX-X-XXXX-XXXX-X [if applicable]

Preface

This report describes the Agricultural Water Use (AWU) Package for MODFLOW or GSFLOW. The program can be downloaded from the USGS for free. The performance of the AWU Package has been tested in a variety of applications. Future applications, however, might reveal errors that were not detected in the test simulations. Users are requested to send notification of any errors found in this model documentation report or in the model program to the contact listed on the Web page (https://doi.org/10.5066/F70C4TQ8). Updates might be made to both the report and to the model program. Users can check for updates on the MODFLOW and GSFLOW Web pages.

Acknowledgments

This research was supported by the U.S. Geological Survey Water Availability and Use Science Program. We appreciate the technical reviews provided by the USGS scientists. Their suggestions resulted in a distinctly better manuscript.

Contents

Abstract 1

Introduction 1

Description of the Modified Footprint Algorithm 3

Initial Redistribution 3

Redistribute to Perimeter Cells when Stalled 4

Using ModelMuse with WellFootprint 4

Starting a New Footprint Project 5

Editing the Grid 5

Non Spatial Data 5

Input Data Sets 6

Running WellFootprint 6

Displaying Results 7

Input file format 7

Output file formats 12

Format of text result file 12

Format of binary results file. 13

Acknowledgments 13

References Cited [or Selected References] 14

Figures

**Figure 1.** Illustration of using proportionally sized circles to represent well withdrawal magnitudes. 2

**Figure 2.** The Footprint is NOT a capture zone, or the area that contributes recharge to the wells. It is solely a visualization of the magnitude of pumping, centered on the wells (Senior and Goode, 2013). 2

**Figure 3.** Steps in the initial redistribution process. *A.* Colored cells are all less than half the distance to the nearest from a withdrawal point to the nearest neighboring withdrawal point are candidate cells. *B.* Cells from A have been eliminated as candidate cells to reduce the sum of the capacities of the candidate cells to less than the associated withdrawal from the withdrawal point. *C.* Candidate cells that lack a path from the withdrawal point through other candidate cells have been eliminated. 4

Agricultural Water Use Package for MODFLOW and GSFLOW

By Richard G Niswonger

# Abstract

The Agricultural Water Use (AWU) Package was developed for simulating water use by agriculture in MODFLOW and GSFLOW models. Previously, simulating agricultural water use in MODFLOW and GSFLOW required external calculations for applying irrigation to model cells or HRUs, making it difficult to link surface water and groundwater supply to applied irrigation amounts. The AWU Package provides additional capabilities not provided by other MODFLOW-based codes used for simulating agricultural water use. For example, the AWU Package calculates irrigation demands, irrigation amounts, evapotranspiration, and return flows that are dependent on dynamic soil-water conditions, and surface water and groundwater availability. Irrigation is explicitly simulated by applying diverted surface water and pumped groundwater to fields. The AWU Package is integrated with the UZF1 and SFR2 Packages for MODFLOW simulations, and it is integrated with the PRMS Soilzone Module and the SFR2 Package for GSFLOW simulations. Surface water diversions simulated by the SFR2 Package can be automatically applied as irrigation to UZF1 cells or PRMS HRUs. Irrigation supplied by groundwater is calculated by the AWU Package, using the same approach as used by the MODFLOW-NWT WELL Package, and pumped groundwater can be automatically applied to UZF1 cells or PRMS HRUs as irrigation. Groundwater irrigation can be the sole source of irrigation water or it can be calculated as the difference between the irrigation demand and surface water diversion when the surface water diversion is less than the irrigation demand for a water right.

# Introduction

Agriculture is a major water-use component in many basins in the western United States, and representation of this water-use sector in hydrologic models is important for water resources planning and management. Conventional approaches for representing water use by agriculture in MODFLOW do not simulate a dynamic soil water balance on farmlands water balance dynamically simulate feedback between supply and demand. For this case, when water supply is less than demand, consumption by agriculture is limited by water supply. Although this approach works well in some settings, there are often cases when agricultural demand is dependent on hydrologic variables that are not known prior to running a hydrologic model, and it is more realistic to calculate demand during a hydrologic simulation, such that feedbacks between supply and demand can be represented more realistically. Irrigation demand is dependent on evolving soil-water conditions on farmlands, as well as, groundwater conditions and return flows, and integrating water use by agriculture into a hydrology model provides capabilities to simulate these processes.

The Agricultural Water-Use (AWU) Package was developed for MODFLOW-NWT and GSFLOW in order to simulate water use for agriculture (Niswonger and others, 2011; Markstrom and others, 2008). The AWU Package works with the Streamflow-Routing (SFR2) and the Unsaturated Flow (UZF1) Packages, and includes capabilities for simulating pumping wells, similar to the WELL Package for MODFLOW-NWT. The AWU Package has 4 major capabilities, including 1) apply water flowing in SFR2 diversion segments as infiltration to UZF1/PRMS cells/HRUs; 2) apply water pumped by wells in the AWU Package as infiltration to UZF1/PRMS cells/HRUs; 3) automatically pump water in wells to supplement SFR2 diversions when the available flow in a diversion segment is less than demand; and 4) calculate irrigation demand using the UZF1/PRMS ET deficit (ETo-ETa). Option 4 includes sub-irrigation where the ET demand can be supplemented by groundwater.

Input required for simulating agricultural diversions, supplementary pumping, irrigation, and demand calculations are all specified within the AWU Package input file. All exchanges between different packages (SFR2, UZF1, and AWU) are calculated within the AWU Package; however, the SFR2 and UZF1 Packages must be active in order to use their capabilities in conjunction with the AWU Package. Diversion segments must be specified within the SFR2 Package in order to apply diverted water as irrigation. All data for supplementary and irrigation wells is specified within the AWU Package input file; the AWU Package calculates and applies its own boundary conditions to the groundwater flow equation for representing groundwater pumping by wells.

The AWU Package can be used to simulate agricultural water use with three different configurations (Figure 1): 1) Surface water diversions are specified in the SFR2 Package and represent irrigation demand, all or a portion of irrigation water is explicitly applied to UZF1 cells or PRMS HRUs and ET and return flows are simulated, or diverted water is removed from the model, assuming complete consumption of diverted water; 2) Surface water diversions are specified in the SFR2 Package or groundwater pumping rates are specified in the AWU Package and represent irrigation demand, or surface water diversions are specified to represent irrigation demand and surface water shortfalls are used to calculate supplementary groundwater pumping, irrigation water is removed from the model assuming complete consumption or is applied to cells/HRUs to simulate ET and return flows; 3) irrigation demand is calculated using the ET deficit in UZF1 or PRMS, and surface water diversions and groundwater pumping rates are calculated by the model and applied to cells/RHUs to minimize the ET deficit, maximum surface water diversions and pumping rates are specified in the SFR2 and AWU Packages, respectively.

The AWU Package is activated by specifying a file type of “AWU” within the MODFLOW-NWT Name file. The AWU input file contains 3 types of data, including 1) Options, 2) Well List, and 3) Stress Period data for specifying connectivity between segments and irrigation cells, supplemental wells and diversion segments, and irrigation wells and irrigation cells.

1. Illustration of using proportionally sized circles to represent well withdrawal magnitudes. Modified from Kresse and others (2014).

The

## Limitation

As The footprint is NOT the area that contributes recharge to the wells. It is solely a visualization of the magnitude of pumping, centered on the wells (Goode, 2016).

# Description of the Modified Footprint Algorithm

The

## Initial Redistribution

The Steps in selecting cells in the initial redistribution process. Around the two wells, (black, solid cells), a neighborhood is selected in which all the cells are active, sufficiently close to the well, and connected by other candidate cells to the well cell.

## Redistribute to Perimeter Cells when Stalled

The

1. Example redistribution to perimeter cells when stalled. Modified from Goode (2016).

# Using ModelMuse with WellFootprint

ModelMuse (Winston, 2009, 2014) has been modified to generate the input for WellFootprint and to display the output from WellFootprint.

## Starting a New Footprint Project

When

## Editing the Grid

If the

## Non Spatial Data

The various

## Input Data Sets

There

## Running WellFootprint

To

1. Extensions Used with WellFootprint Files

|  |  |
| --- | --- |
| WellFootprint File type | Extension |
| Input | .fpi |
| Listing | .fplst |
| Binary results | .fpb |
| Text results | .fpt |

## Displaying Results

To d

# WellFootprint Input file format

An e

# WellFootprint Output file formats

## Format of text result file

The text result file contains two arrays Distributed\_Withdrawals and Footprint\_Code (table 2).

1. The data for each array starts with a line containing the name of the array.
2. This is followed by two lines containing the number of rows and number of columns in the grid respectively.
3. This is followed by a value for each cell in the grid in row-major order. Commas and white space are used to separate values.
4. Meaning of Footprint Codes

|  |  |
| --- | --- |
| Footprint code | Meaning1 |
| 0 | Inactive |
| 1 | Q = 0 |
| 2 | 0 < Q < D |
| 3 | Q = D |
| 4 | Q > D |

1 Q = Withdrawal rate; D = Cell capacity

## Format of binary results file.

# Discussion

While the use of WellFootprint to display well withdrawals has been emphasized here, there are other sorts of data that could be displayed using WellFootprint. For instance, disease frequency could be displayed to create maps that are easier to understand. In general, the footprint method might be useful when plotting any type of closely spaced point data of varying intensity.

# References Cited

Goode, D.J., 2016, Map visualization of groundwater withdrawals at the sub-basin scale: Hydrogeology Journal, v. 24, no. 4, p. 1057-1065.

ISSN (online)  
http://dx.doi.org/x